{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":5,"rows_kept":4,"merged":[[0,0,1,0],[2,0,3,0],[4,0,5,0]]}
[1,"设备名称","数量","服务年限","技术参数"]
[null,"全院氧气负压系统运维服务",1,"1年"]
[2,"设备名称","数量","预算单价\n（万）","技术参数"]
[null,"输液泵",2,2.4,"1. 输液精度≤±5%\n2. 预置输液总量范围：0.1-9999.99ml\n3. 快进流速范围：0.1-2300ml/h，具有自动和手动快进可选；\n4. 在线动态压力监测，可实时显示当前压力数值；\n5.具备单个气泡和累积气泡报警功能，支持最小15μL的单个气泡报警\n6. 无需滴数传感器，泵可自动识别空瓶状态并报警"]